|  |  |  |  |
| --- | --- | --- | --- |
| **Chanel** | **Instrument** | **Mic/Direct Box1** | **Insert (Drawmer, KlarkTeknik, BSS, XTA, DBX, PreSonus)** |
| 1 | djembe -top | SHURE-56-57, Sennheiser-E604-904, Electro-Voice-PL35, AUDIX-OM5 | Compressor +Gate |
| 2 | djembe -bot | SHURE-52-56-57,AKG-112, AUDIX-D6-OM5, Sennheiser-E604-904, Electro-Voice-PL35 | Compressor +Gate |
| 3 | darbuka-top | SHURE-56-57, Sennheiser-E604-904, Electro-Voice-PL35, AUDIX-OM5 | Compressor +Gate |
| 4 | darbuka-bot | SHURE-56-57, Sennheiser-E604-904, Electro-Voice-PL35, AUDIX-OM5 | Compressor +Gate |
| 5 | voc-women | SHURE-58, AUDIX-OM7, SENNHEISER-E935 | Compressor |
| 6 | voc-man | SHURE-58, AUDIX-OM7, SENNHEISER-E935 | Compressor |
| --- | voc-man-back | SHURE-58, AUDIX-OM7, SENNHEISER-E935 |  |
| 7 | flute | SHURE-57-58, AUDIX-OM5-OM7,  SENNHEISER-E935 |  |
| 8 | didjeridoo | SHURE-52-56-57,AKG-112, AUDIX-D6-OM5,Sennheiser-E604-904, Electro-Voice-PL35 |  |
| 9 | cello | DI-BOX | Compressor |
| 10 | bass | DI-BOX | Compressor |
| 11 | sampler-L | DI-BOX |  |
| 12 | sampler-R | DI-BOX |  |
| 13 | synth-focusrite-L | DI-BOX |  |
| 14 | synth-focusrite-R | DI-BOX |  |
| 15 | talk back | Any microphone |  |
| 16 | PLATE-REVERB | stereo | time/decay/size |
| 17 | DELAY | stereo | Tap |